11000001:Device
11000043:BSD Log Device
12000002:Path
12000004:Description
12000005:Locale
12000016:Debug Target Name USB
12000019:Debug Bus Parameters
1200001D:Debug Net Key
12000030:Load Options String
12000044:BSD Log Path
1200004A:Font Path
14000006:Inherited Objects
14000008:Recovery Sequence
15000007:Truncate Memory
1500001A:Debug Host IP
1500001B:Debug Net Port
1500000C:First MB Policy
1500000D:Relocate Phy Memory
1500000E:Avoid Low Phy Memory
15000011:Debug Type
15000012:Debug Serial Port Addr
15000013:Debug Serial Port
15000014:Debug Baud Rate
15000015:Debug 1394 Channel
15000018:Debug Start Policy
15000022:EMS Port
15000023:EMS Baud Rate
15000042:Key Ring Address
15000047:Config Access Policy
1500004B:Integrity Services
1500004C:Volume (FVE) Band ID
15000051:Initial Console Input
15000052:Graphic Resolution
15000065:Display Message
15000066:Display Message Override
1500006D:Boot UX Fade Frames
15000073:Alias Win Key
15000075:Perf Freq
15000076:Secure Boot Raw Policy
15000079:Boot UX Transision Time
1500007D:Boot Error UX
1500007F:Measured Boot Log Format
15000081:Log Control
16000009:Recovery Enabled
1600000B:Bad Mem Access Allowed
1600000F:Traditional KSeg
16000010:Boot Debug Enabled
16000017:No UMEX
1600001C:Debug DHCP
1600001E:VM
16000020:Boot EMS
16000031:Attempt Non BCD Start
16000040:Advanced Options
16000041:Options Edit
16000045:Preserve Boot Stat
16000046:Graphics Mode Disabled
16000047:Config Access Policy
16000048:No Integrity Checks
16000049:Test Signing
16000050:Extended Input
16000053:Restart On Failure
16000054:Highest Graphic Mode
16000060:Isolated Exe Context
16000067:No Boot UX Logo
16000068:No Boot UX Text
16000069:No Boot UX Progress
1600006A:No Boot UX Fade
1600006B:Boot UX Reserve Pool Dbg
1600006C:Boot UX Disable
1600006E:Boot UX Dump Stats
1600006F:Boot UX Show Stats
16000071:Multiboot System
16000072:No Keyboard
16000074:Boot Shutdown Disabled
1600007A:Mobile Graphics
1600007B:Force FIPS Crypto
1600007E:Flight Signing
1700000A:Bad Memory List
17000077:Allowed in Mem Settings
25000510:Charge Threshold
25000AAA:Boot Flow
26000202:Skip FFU Mode
26000203:Force FFU Mode
26000512:Off Mode Charging
{bootmgr}{fwbootmgr}{any}{app}***
21000022:BCD Device
22000023:BCD File Path
22000026:PW Override
22000027:Pinpass Phrase Override
22000040:FVE Recovery URL
22000041:FVE Recovery Message
23000003:Default
23000006:Resume Object
24000001:Display Order
24000002:Boot Sequence
24000010:Tool Display Order
25000004:Timeout
26000005:Resume
26000020:Display Boot Menu
26000021:No Error Display
26000024:Horm Enabled
26000025:HiberBoot
26000028:Process Custom Actions First
26000031:Persist Boot Sequence
27000030:Custom Actions List
{osloader}{any}{app}***
21000001:OS Device
21000138:IMC Device
21000150:System Data Device
22000002:System Root
22000011:Kernel Path
22000012:HAL Path
22000013:Debug Transport
22000053:EVStore
220000F1:Hypervisor Path
220000f9:Hypervisor Debug Bus Params
22000110:Hypervisor Debug Net Key
22000112:Hypervisor Product SKU Type
22000117:Hypervisor Load Options
2200012D:Kernel Bus Params
22000132:Kernel Debug USB Target Name
22000136:Kernel Debug Net Key
22000137:IMC Hive Name
22000140:MFG Mode
23000003:Resume Object
25000020:NX Policy
25000021:PAE
25000031:Remove Memory
25000032:Increase User VA
25000033:Performance Memory
25000050:Cluster Mode Addressing
25000052:Restrict APIC Cluster
25000055:X2 APIC Policy
25000061:Num CPU
25000063:Config Flags (CPU)
25000066:Group Size
25000071:MSI
25000072:PCI Express
25000080:Safe Boot
250000A6:TSC Sync Policy
250000C0:Force Failure
250000C1:Driver Load Failure Policy
250000C2:Boot Menu Policy
250000E0:Boot Status Policy
250000F0:Hypervisor Launch Type
250000F3:Hypervisor Debug Type
250000F4:Hypervisor Debug Port Num
250000F5:Hypervisor Debug Baud
250000F6:Hypervisor Debug 1394 Channel
250000F7:Boot Ux Policy
250000FA:Hypervisor Num CPU
250000FB:Hypervisor Root CPU Per Node
250000FD:Hypervisor Debug Host IP
250000FE:Hypervisor Debug Host Port
250000FF:Hypervisor Debug Pages
25000100:TPM Boot Entropy Policy
25000113:Hypervisor Root CPU
25000115:Hypervisor IOMMU Policy
25000118:Hypervisor MSR Filter Policy
25000119:Hypervisor MMIO NX Policy
25000120:XSave Policy
25000121:XSave Add Feature 0
25000122:XSave Add Feature 1
25000123:XSave Add Feature 2
25000124:XSave Add Feature 3
25000125:XSave Add Feature 4
25000126:XSave Add Feature 5
25000127:XSave Add Feature 6
25000128:XSave Add Feature 7
25000129:XSave Remove Feature
2500012A:XSave CPU Mask
2500012B:XSave Disable
2500012C:Kernel Debug Type
2500012E:Kernel Debug Address
2500012F:Kernel Debug Port
25000130:Claimed TPM Counter
25000131:Kernel Debug 1394 Channel
25000133:Kernel Debug Host IP
25000134:Kernel Debug Net Port
25000139:Kernel Debug BAUD Rate
25000142:VSM Launch Type
25000144:Hypervisor Enforced Code Integrity
26000004:Stamp Disks
26000010:Detect Hal and Kernel
26000022:WinPE
26000024:No Crash Auto Reboot
26000025:Last Known Good Config
26000026:OSL No Integrity Checks
26000027:OSL Test Signing
26000030:No Low Mem
26000040:VGA Mode
26000041:Quiet Boot
26000042:No VESA
26000043:No VGA Mode
26000051:Use Physical Destination
26000054:Use Legacy APIC Mode
26000060:One CPU
26000062:Max CPU
26000064:Max Group
26000065:Group Aware
26000070:Use FW PCI Settings
26000081:Safe Boot Alt Shell
26000090:Boot Log Init
26000091:SOS
260000A0:Debug Kernel Enable
260000A1:HAL Breakpoint
260000A2:Use Platform Clock
260000A3:Force Legacy Platform
260000A4:Use Platform Tick
260000A5:Disable Dynamic Tick
260000B0:EMS
260000C3:One Time Advanced Options
260000C4:One Time Options Edit
260000E1:Disable ELAM Drivers
260000F2:Hypervisor Debug Enable
260000F8:Hypervisor Disables LAT
260000Fc:Hypervisor Use Large VTLB
26000114:Hypervisor Debug DHCP
26000116:HyperVisor Use VAPIC
26000135:Kernel Debug DHCP
26000141:Event Logging
{resume}{any}{app}***
21000001:File Device
21000005:Assoicated OS Device
22000002:File Path
25000007:Boot UX
25000008:Boot Menu Policy
26000003:Custom Settings
26000004:PAE
26000006:Debug Option Enabled
26000024:Horm Enabled
{device}{any}***
31000003:Ram Disk DI Device
32000004:Ram Disk DI Path
35000001:Ram Disk Image Offset
35000002:Ram Disk TFTP Client Port
35000005:RAM Disk Image Length
35000007:RAM Disk TFTP Block Size
35000008:RAM Disk TFTP Window Size
36000006:RAM Disk Export as CD
36000009:RAM Disk Multicast Enable
3600000a:RAM Disk Multicast TFTP Fallback
3600000b:RAM Disk TFTP Var Window
{memdiag}{any}{app}***
25000001:Pass Count
25000002:Test Mix
25000003:Fail Count
25000004:Test To Fail
25000005:Stride Fail Count
25000006:Invc Fail Count
25000007:MATS Failure Count
25000008:RAND Failure Count
25000009:Chckr Fail Count
26000003:Cache Enabled (6.2+)
26000004:Failures Enabled
26000005:Cache Enable (6.1)
{ntldr}{any}{app}***
22000001:BPB String
{osloader}{setupldr}{any}{app}***
42000002:App Relative Path
42000003:Ramdisk Device Relative Path
45000001:Device Type
46000004:Omit OS Loader Elements
46000010:Recovery OS
47000006:Elements to Migrate
{startup}{any}{app}***
26000001:PXE Soft Reboot
22000002:PXE App Name
